#!/usr/bin/env bash
#
# Build tests for SAMD21 (Minitronics 2.0)
#

# exit on first failure
set -e

#
# Build with the default configurations
#
restore_configs
opt_set MOTHERBOARD BOARD_MINITRONICS20 SERIAL_PORT -1 \
        TEMP_SENSOR_0 11 TEMP_SENSOR_BED 11 \
        X_DRIVER_TYPE DRV8825 Y_DRIVER_TYPE DRV8825 Z_DRIVER_TYPE DRV8825 E0_DRIVER_TYPE DRV8825 \
        RESTORE_LEVELING_AFTER_G28 false \
        LCD_LANGUAGE it \
        SDCARD_CONNECTION LCD \
        HOMING_BUMP_MM '{ 0, 0, 0 }'
opt_enable ENDSTOP_INTERRUPTS_FEATURE BLTOUCH Z_MIN_PROBE_REPEATABILITY_TEST \
           FILAMENT_RUNOUT_SENSOR G26_MESH_VALIDATION MESH_EDIT_GFX_OVERLAY Z_SAFE_HOMING \
           EEPROM_SETTINGS NOZZLE_PARK_FEATURE SDSUPPORT SD_CHECK_AND_RETRY \
           REPRAPWORLD_GRAPHICAL_LCD ADAPTIVE_STEP_SMOOTHING \
           STATUS_MESSAGE_SCROLLING SET_PROGRESS_MANUALLY SHOW_REMAINING_TIME SET_REMAINING_TIME \
           LONG_FILENAME_HOST_SUPPORT CUSTOM_FIRMWARE_UPLOAD M20_TIMESTAMP_SUPPORT \
           SCROLL_LONG_FILENAMES BABYSTEPPING DOUBLECLICK_FOR_Z_BABYSTEPPING \
           MOVE_Z_WHEN_IDLE BABYSTEP_ZPROBE_OFFSET BABYSTEP_ZPROBE_GFX_OVERLAY \
           LIN_ADVANCE ADVANCED_PAUSE_FEATURE PARK_HEAD_ON_PAUSE MONITOR_DRIVER_STATUS SENSORLESS_HOMING \
           SQUARE_WAVE_STEPPING EXPERIMENTAL_SCURVE
exec_test $1 $2 "Minitronics 2.0 with assorted features" "$3"

# clean up
restore_configs
