---
name: Bug report
about: Create a report to help us improve
title: "[BUG]"
labels: bug
assignees: ''

---

<!--

Before posting a bug report, make sure to thoroughly read the readme and Wiki. 
https://github.com/davidramiro/Marlin-AI3M/wiki/

I am happy to help everyone as much as I can, but make sure your bug report is only applicable to this specific firmware.
Example of a valid bug report: "M600 filament change is not working as expected."
Example of an invalid request: "I am powering my printer with a hamster wheel generator. It's not working properly. Fix pls."

-->

**Describe the bug**
A clear and concise description of what the bug is.

**To Reproduce**
Steps to reproduce the behavior:
1. Start printer
2. Move axis by '....'
3. Start printing '....'
4. See error

**Expected behavior**
A clear and concise description of what you expected to happen.

**Photos of the print / output of the terminal**
If applicable, add photos or console outputs to help explain your problem.

**Printer (please complete the following information):**
 - Firmware version: [e.g. v19.02.08]
 - Printing method [e.g. SD, USB (OctoPrint, Cura, ...)]
 - Model [e.g. i3 Mega, Mega-S]

**M503 Output**
Please paste the complete output of the `M503` command here.
